Important Information!

- When running your new frequency generator together with a Rife/Bare system or other strong RF generating devices follow these guidelines:

1) make sure you install ferrite filters on all cables going to the generator including the cable that connects to the BNC output connector on the generator. This will prevent lockups or other problems due to RF interference. Our generators come with a ferrite pre-installed on the wall transformer cable. But in some very powerful systems, it may be necessary to add more ferrites to this cable. Install the ferrite(s) as close as possible to the existing ferrite and wrap as many turns as will fit in the ferrite(s). Our generators are very well shielded against RF interference. They have a 6 layer PCB with dedicated ground and power planes. But the cables are the weak link in such a system. They act like antennas and need to be protected against RF emissions. In such a system, it is better to run the generator standalone with the USB cable disconnected. Good sources for ferrites are:

www.allelectronics.com

www.digikey.com

www.radioshack.com part number 273-105

2) Keep all objects away from the keypad. Do not wrap wires (including the power wire) around the generator case. Keep wires away from the keypad.

3) Keep the generator and the wall transformer as far away from the plasma tube as possible. Keep a distance of at least 3 feet between the generator-wall transformer-power cable and the plasma tube.

4) If after following the guidelines above you still have problems running the generator while the plasma tube is running, you can have the generator disable the keypad while running a program by setting the option "No keys at run" to 1 in the preferences: From the keypad, touch "menu" and scroll up to "Preferences" and touch "enter". Touch "bksp" and touch "1", touch "enter" and "enter" again. This will disable the keypad only while a program runs. You will not be able to use the keypad until the program is done running but this should allow the generator tu run a program even while a Plasma tube is running.